Power rating

|  |  |  |
| --- | --- | --- |
|  | Jetson Nano | Jetson Xavier NX |
| Voltage in | 5V | 19V |
| Voltage usage | 5V | 5V |
| Power | Max 10W | Max 20W |
| Max rated current | 5A | 5A |
| Power method | Power jack, usb, gpio header | Power jack |